\***PRODUCT INFORMATION SHEET**

**ALKALINE DRAIN CLEANER 30%**

**(Caustic Soda 30% (w/w))**

**PRODUCT DESCRIPTION:**

A caustic soda based highly efficient grease eater. To be used in toilets, drains, traps, etc. Not suitable for aluminium based fittings.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**ADVANTAGES:**

HIGHLY CONCENTRATED: Alkaline Drain Cleaner contains caustic soda, a powerful grease cutting agent which quickly liquefies grease, fat, organic matter and

 sludge, enabling drains and pipes to flow freely.

QUICK ACTING: Alkaline Drain Cleaner starts to work immediately upon application.

LIQUID PRODUCT: Being a liquid Alkaline Drain Cleaner is easier and safer to use, than some of the powdered products.

EASY TO RINSE: After Alkaline Drain Cleaner has freed the black artery simply pour copious amounts of water down the artery.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**DIRECTIONS FOR USE:**

Pour undiluted Alkaline Drain Cleaner down the blocked pipe, drain etc. Leave to work for about 15 minutes. Rinse down the drain with copious amounts of water. Not suitable for aluminium based fittings. Do not mix with other cleaners, particularly acid based cleaners.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**HEALTH AND SAFETY:** See Safety Data Sheet.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**PACKAGING:**

All our plastic drums are high molecular weight, high density polyethylene designed to bring the product to the customer in perfect conditions.

Size: 5 Lt. Drums, 25 Lt. Drums.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_